                                  ZEROPLUS Protocol Analyzer MIPI DSI Module_Ver1.02.00
  Date:2013/7/16                                  ZEROPLUS Technology CO;TD 
//////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////

            Thank you for purchasing Zeroplus Logic Analyzer.
      For this package, it includes installation of ZEROPLUS Protocol Analyzer MIPI DSI Module_Ver1.02.00.
      Following readme information will help you know the features of ZEROPLUS Protocol Analyzer MIPI DSI Module.


     Index
      ================================
         1. Features
         2. System Requirements
         3. ZEROPLUS Protocol Analyzer MIPI DSI Module Installation
         4. Notice issues
	 5. Contact information
      ================================
     1. Features
	  MIPI Alliance (www.mipi.org) was established together by ARM, Nokia, ST, TI and other
        companies in 2003. It aims at standardizing the internal interfaces of mobile phone, such
        as cameral interface, display interface, RF/baseband interface, etc., so as to simplify
        the mobile phone design and increase the design flexibility. Under the MIPI Alliance 
        there are many WorkGroups, each WorkGroup defines a internal interface standard for 
        mobile phone, such as cameral interface (CSI), display interface (DSI), Dig RF, 
        microphone/loudspeaker interface (SLIM bus), etc.. With the interface standard unified, 
        mobile phone manufacturers can select different chips and modules as their requirements  
        from the market, and modify the mobile phone¡¦s design and function more conveniently.

     2. System Requirements
        
          Operation System:
             Windows 2000 (Professional & Server series).
             Windows XP (Home & Professional Editions 32-Bit version).
             Windows Vista (32-Bit and 64-Bit version).
             Windows 7 (32-Bit and 64-Bit version).

          Hardware System Requirements:
          CPU:
             166MHz (Lowest Configuration), or above 900MHz (Recommended Configuration).
 
          Memory Size:
             64MB or above (Lowest Configuration).
             256MB or above (Recommended Configuration).

          Display Device:
             VGA Display Capability with 1024x768 resolution or higher.
 
          Disk Space:
            At least 100MB available disk space. 

          USB:
            USB1.1 compatible (Lowest Configuration); USB2.0 compatible (Recommended Configuration).

     3. To install ZEROPLUS Protocol Analyzer MIPI DSI Module on a computer:
         3.1. Insert the disk of ZEROPLUS Protocol Analyzer MIPI DSI Module on CD-ROM drive, follow these steps.
              Auto-installation is running, click "START installing ZEROPLUS Protocol Analyzer MIPI DSI" on the 
              options menu. 
              If Auto-installation is not running, Go to the START menu, click START, click Run, click Browse to Locate 
              the root folder of the ZEROPLUS Protocol Analyzer MIPI DSI location, select Setup.exe file to start 
              installation.
         3.2. During installation, click "I accept " on the authorized agreement and then continue installation.
              If you don¡¦t accept the conditions written on the agreement, click "I don¡¦t accept " to cancel 
              installation.
         3.3. After executing Logic Analyzer software, click right-key to select "Gather signal Lines being a bus". 
              Then move cursor to the location of "added new bus" and click right-key to select "Bus property". 
              Click "Protocol Analyzer settings" and the functional option of ZEROPLUS LA MIPI DSI are on the 
              list. Selected this option and go to Parameter Settings, typing the value to start the analysis of LED 
              Pitch Array.
              
     4. Notice issues
         4.1. Protocol Analyzer is available only after installing ZEROPLUS Logic Analyzer program.
         4.2. For register, please contact our sales.
         4.3. Modify Item:
            4.3.1. Add notice of failed decoding caused by wrong packet format.

     5.Contact information: 
            Service days Monday to Friday, Am 9:00-12:00/PM 1:30-5:30
            ZEROPLUS technology co; LTd.

            Headquarter
            Address: 3F., No.121, Jian 8th Rd., Zhonghe Dist., New Taipei City 23585, Taiwan (R.O.C.)
            Tel:   886-2-6620-2225 
            Fax:   886-2-6620-2226

            Instrument Business / Sales department 
            Address: 2F., No.123, Jian 8th Rd., Zhonghe Dist., New Taipei City 23585, Taiwan (R.O.C.)
            Service phone: 886-2-6620-2225  Extension: 200
            Fax:	  886-2-2223-4362
            Service mail: service_2@zeroplus.com.tw

            Instrument Business /Taiwan-Hsinchu
            Address: 2F., No.242-1, Nanya St., North Dist., Hsinchu City 30052, Taiwan (R.O.C.)
            Service phone: 886-3-5426637 	Extension: 87
            Fax:           886-3-5424917
            Service mail: hunter@zeroplus.com.tw

            Instrument Business / China-Beijing
            Address:Room 402, Block D, Building 13, Courtyard 9(Dangdai City Jiayuan), Anningzhuang
            West Road, Haidian District, Beijing
            Service phone: +86-10-51159268 
            Fax:           +86-10-51159278 
            Service mail: adam1833@zeroplus.com.tw
                          kan@zeroplus.com.tw

            Instrument Business / China-Shanghai
            Address:Room 101, 8th Building, Lane 825, Chen Hui Road, Zhangjiang District, Pudong New 
            Area, Shanghai City
            Service phone: +86-21-50155235 ~6
            Fax:           +86-21-50155235  #607
            Service mail: adam1833@zeroplus.com.tw
                          kan@zeroplus.com.tw
           
            Instrument Business / China-Shenzhen	
            Address:Room 605, Huameiju C District, Huafeng Sci.&Tech. Park, Xinhu Road, 82 Zone, Bao'an,
            Shenzhen  
            Service phone: +86-755-2955-6305 ~6
            Fax:           +86-755-2955-6306  #613
            Service mail: jesse_cn@zeroplus.com.tw
                          kan@zeroplus.com.tw

            The website of Zeroplus: www.zeroplus.com.tw

            Copyright 2013, ZEROPLUS Technology CO;LTD
            All  other brands & product names are other company & organization's trade mark or registered trade mark.